170 - List of material and assembly information

3D printable housing:

As printing material you can use standard PLA in a colour of your choice. We used 25% percent infill for the print. 
A standard 3D-printer with 24x24 cm plane is sufficient.

Loudspeakers and cabling:

1 x SB Acoustics SB17CRC35-4 6’’ 
7 x Fountek FE88EX 3"
2 x Neutrik NL8MPR
ca. 3.5m strand
8 x 2.8mm  blade receptacle
24 x 4.8mm blade receptacle

Loudspeaker/NL8 mounting + housing connection

40 x (3.5mm x 3cm) bolt
4 x (3.5mm x 4.5cm) bolt
44 x 3.5mm square nut
44 x (3.5mm / 7mm) washer
44 x 3.5mm lock washer

Flange:

1 x Adam Hall SM720 (threaded flange)
4 x nuts
4 x bolts

Extras:

- We used foam tape to minimise vibrations between loudspeakers and housing as well as between the two housing parts.
- Using a 3D pen the nuts can be fixated inside the housing (useful for changing loudspeakers).

Suggested Amplifier:

Monacor STA-850D (~350 €)